
Standard Operating Procedure (SOP)

	1.
	Contact Information

	Procedure Title:
	ARC FLASH Event

	Division:
	Bus Maintenance 

	Department/Function:
	[Specify]
	SOP number:
	[Specify]

	Prepared by:
	CALSTART
	Date:
	1/6/2023
	Date issued:
	[Specify]

	Reviewed by:
	[Specify]
	Date:
	[Specify]
	Revision date:
	[Specify]

	Approved by:
	[Specify]
	Date:
	[Specify]
	Review date:
	[Specify]




	2.
	Purpose

	Overview of ARC FLASH Event: an event that results from a connection through air to ground or another voltage phase in an electrical system.




	3.
	Scope

	Cover First Person/Responder on Scene from vehicle ARC FLASH Event.











	4.
	Responsibility

	First on scene, Supervisor.  Identified in the Step-By-Step Operating Procedure.
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	5.
	Definitions

	AED – Automatic External Defibrillator



	[bookmark: _Hlk32497515][bookmark: _Hlk32497606]6.
	Prerequisites (Training Requirements)

	None.


[bookmark: _Hlk32505565]
	7.
	Step-By-Step Operating Procedure

		Responsible Party
	Action Step

	**** DO NOT TOUCH PERSON STILL IN CONTACT WITH SOURCE OF ELECTRICAL SHOCK *****

	




First on Scene
	1. If person is still in contact with electrical source, use a dry, non-conducting object, such as a wooden broom, chair, or hot stick to eliminate person’s contact with electrical source.


	
	2. If safe to do so, turn off power source by switching off the Battery Disconnect switch to OFF position (IMG 1.0).


	
	3. Turn the High Voltage Disconnect Switch to OFF Position (IMG 1.0).

	
	4. Check to see if person is breathing.


	
	5. If they are breathing, 
A. Contact 911 first always.
6. If they are not breathing.
A. Designate a person to call 911.
B. Begin CPR and utilize an AED (Manual Defibrillator) and continue until Emergency Services arrives.

	
	7. If victim is on fire, flames can be smothered or doused. 
DO NOT REMOVE CLOTHES FROM VICTIM!
Smother example:  Cover with a blanket or jacket.
Douse example:  Use water to extinguish fire.

	
	8. Report Incident to Supervisor once Emergency Services has arrived and taken over if a Supervisor has not already 
been alerted.









	7.
	Step-By-Step Operating Procedure (continued)

		Responsible Party
	Action Step

	**** DO NOT TOUCH PERSON STILL IN CONTACT WITH SOURCE OF ELECTRICAL SHOCK *****

	



Supervisor
	1. Ensure person is no longer in contact with electrical source of shock. If still in contact, use a dry, non-conducting object, such as a wooden broom, chair, or hot stick to eliminate person’s contact with electrical source. DO NOT ASSUME THIS HAS BEEN DONE!


	
	2. Verify with First Person on Scene the Battery Disconnect switch has been switched to the OFF position (see IMG 1.0).


	
	3. Verify with First Person on Scene that 911 have been called and follow 911 operator instructions.


	
	4. If person is showing signs of shock, such as vomiting or becoming faint or very pale, elevate the legs slightly, unless this causes too much pain.


	
	5. If possible, cover burns with sterile gauze. DO NOT USE ADHESIVE BANDAGES THAT MAY STICK TO THE BURN.


	
	6. Keep the person warm using available materials. (Example: blankets, jackets, coats)




	
	7. Await rescue worker / EMT instruction.




















	8.
	Equipment & Materials

	    
    
      TBD from Manufacturer
               IMG 1.0



	9.
	Health & Safety

	None.


     
	[bookmark: _Hlk32498206]10.
	Waste Disposal

	None.



	11.
	Quality Assurance & Quality Control

	None.




image1.jpg
CRLSTRRT





